|  |
| --- |
| **Protecting the Coastline – Hard & Soft Engineering Approaches** |

|  |  |  |  |
| --- | --- | --- | --- |
| Image | How it works | Advantage | Disadvantage  |
|  | Groyne: Wooden barrier aimed at blocking the movement of beach sediment by LSD. Traps sand on the updrift side of the groyne.  | Very effective and preserved beach sediment therefore protecting tourism economy of seaside resorts.  | Very costly. €230,000 per wooden groyne. Wood decays over time. May be unsightly and dangerous (Mr P story).  |
|  |  |  |  |
|  |  |  |  |